,Wattage##ELECTRICAL_WATTAGE##WATTS,Voltage Loss##OTHER##,Total Light Loss Factor##OTHER##,Tilt Angle##ANGLE##DECIMAL DEGREES,Temperature_W##OTHER##,Temperature_N##OTHER##,Temperature Loss##OTHER##,Temperature Color##OTHER##,Table##OTHER##,T##LENGTH##MILLIMETERS,Temperature_M##OTHER##,Surface Depreciation Loss##OTHER##,Photometric Web File##OTHER##,OLV_Code##OTHER##,URL##OTHER##,None##OTHER##,Luminous Intensity##ELECTRICAL_LUMINOUS_INTENSITY##CANDELAS,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Luminaire Dirt Depreciation##OTHER##,Light Loss Input Method##OTHER##,Light Loss Factor##OTHER##,Lamp Tilt Loss##OTHER##,Lamp Lumen Depreciation##OTHER##,Initial Light Intensity Input Method##OTHER##,Initial Intensity##OTHER##,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Initial Color##OTHER##,Illuminance##ELECTRICAL_ILLUMINANCE##LUX,Emit from Circle Diameter##LENGTH##MILLIMETERS,Emit Shape Visible in Rendering##OTHER##,Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT,Dimming Lamp Color Temperature Shift##OTHER##,Color Filter##OTHER##,Ballast Loss##OTHER##,OLV_Type##OTHER##,OLV_Temperature##OTHER##,OLV_Supply##OTHER##,OLV_Supplementary_Description##OTHER##,OLV_Price##CURRENCY##CURRENCY,OLV_Power##OTHER##,OLV_Nominal lumen##OTHER##,OLV_Disclaimer##OTHER##,OLV_Composed_by##OTHER##,OLV_Code_Type##OTHER##,OLV_CRI##OTHER##,Model##OTHER##,Manufacturer##OTHER##,C##LENGTH##MILLIMETERS,Description##OTHER##,At a distance##LENGTH##MILLIMETERS,Actual Cable length##LENGTH##MILLIMETERS,Cable length##LENGTH##MILLIMETERS,B##LENGTH##MILLIMETERS
M,9.290304000000,1,1,90.000000000000,0,0,1,0,Oleve_9392,100.000000000000,1,1,generic,9392M-NO-NO,https://www.olevlight.com/categorie-prodotti/,,109.816910733408,1380.000000000000,1,0,,1,1,0,,2700.000000000000,,11.820593893742,609.600000000000,0,148.541963750594,0,16777215,1,"sospensione
",M, 220-240V,"1x5.8W, 220-240V, 2700K- Canopy Super-matt black| Body Super-matt black",589.000000000000,1x5.8W
,1x515lm,"The BIM object is a non-detailed graphical representation of the product. For further details, updates, and design confirmations, please contact the technical office.",RS03/02-NO + 9301M-NO,"Assembly
",>90,,Olev,2.000000000000,SHINE VERTICAL PLUMAGE,3048.000000000000,1200.000000000000,1200.000000000000,2.000000000000
W,9.290304000000,1,1,90.000000000000,1,0,1,0,Oleve_9392,200.000000000000,0,1,generic,9392W-OS-BV,https://www.olevlight.com/categorie-prodotti/,,109.816910733408,1380.000000000000,1,0,,1,1,0,,3000.000000000000,,11.820593893742,609.600000000000,0,148.541963750594,0,16777215,1,"sospensione
",W, 220-240V,"1x5.8W, 220-240V, 3000K- Canopy Brushed brass| Body Painted burnished",589.000000000000,1x5.8W
,1x515lm,"The BIM object is a non-detailed graphical representation of the product. For further details, updates, and design confirmations, please contact the technical office.",RS03/02-OS + 9301W-BV,"Assembly
",>90,,Olev,1.000000000000,SHINE VERTICAL PLUMAGE,3048.000000000000,1500.000000000000,1500.000000000000,3.000000000000
N,9.290304000000,1,1,90.000000000000,0,1,1,12,Oleve_9392,300.000000000000,0,1,generic,9392N-NO-NO,https://www.olevlight.com/categorie-prodotti/,,109.816910733408,1380.000000000000,1,0,,1,1,0,,4000.000000000000,,11.820593893742,609.600000000000,0,148.541963750594,0,16777215,1,"sospensione
",N, 220-240V,"1x5.8W, 220-240V, 4000K- Canopy Super-matt black| Body Super-matt black",589.000000000000,1x5.8W
,1x515lm,"The BIM object is a non-detailed graphical representation of the product. For further details, updates, and design confirmations, please contact the technical office.",RS03/02-NO + 9301N-NO,"Assembly
",>90,,Olev,2.000000000000,SHINE VERTICAL PLUMAGE,3048.000000000000,1500.000000000000,1500.000000000000,2.000000000000
