,Wattage##ELECTRICAL_WATTAGE##WATTS,Voltage Loss##OTHER##,Total Light Loss Factor##OTHER##,Tilt Angle##ANGLE##DECIMAL DEGREES,Temperature_W##OTHER##,Temperature Loss##OTHER##,Temperature Color##OTHER##,Table##OTHER##,T##LENGTH##MILLIMETERS,Temperature_M##OTHER##,Surface Depreciation Loss##OTHER##,Photometric Web File##OTHER##,OLV_Code##OTHER##,None##OTHER##,Luminous Intensity##ELECTRICAL_LUMINOUS_INTENSITY##CANDELAS,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Luminaire Dirt Depreciation##OTHER##,Light Loss Input Method##OTHER##,Light Loss Factor##OTHER##,Lamp Tilt Loss##OTHER##,Lamp Lumen Depreciation##OTHER##,Initial Light Intensity Input Method##OTHER##,Initial Intensity##OTHER##,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Initial Color##OTHER##,Illuminance##ELECTRICAL_ILLUMINANCE##LUX,Emit from Circle Diameter##LENGTH##MILLIMETERS,Emit Shape Visible in Rendering##OTHER##,Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT,Dimming Lamp Color Temperature Shift##OTHER##,Color Filter##OTHER##,Ballast Loss##OTHER##,At a distance##LENGTH##MILLIMETERS,URL##OTHER##,OLV_Type##OTHER##,OLV_Temperature##OTHER##,OLV_Supply##OTHER##,OLV_Supplementary_Description##OTHER##,OLV_Price##CURRENCY##CURRENCY,OLV_Power##OTHER##,OLV_Nominal lumen##OTHER##,OLV_Disclaimer##OTHER##,OLV_Composed_by##OTHER##,OLV_Code_Type##OTHER##,OLV_CRI##OTHER##,Model##OTHER##,Manufacturer##OTHER##,G##LENGTH##MILLIMETERS,Description##OTHER##,Actual Cable length##LENGTH##MILLIMETERS,C##LENGTH##MILLIMETERS,Cable length##LENGTH##MILLIMETERS,B##LENGTH##MILLIMETERS
M,9.290304000000,1,1,60.000000000000,0,1,0,Oleve_2627,100.000000000000,1,1,generic,2627M-BV-BV-BAM,,109.816910733408,1380.000000000000,1,0,,1,1,0,,2700.000000000000,,11.820593893742,350.000000000000,0,148.541963750594,0,16777215,1,3048.000000000000,https://www.olevlight.com/categorie-prodotti/,"sospensione
",M,220-240V,"1x13.8W, 1x6.1W, 220-240V, 2700K- Canopy Painted burnished| Body Painted burnished| Glass Glass: Balloton amber",1230.000000000000,"1x13.8W, 1x6.1W","1x1880lm, 1x669lm","The BIM object is a non-detailed graphical representation of the product. For further details, updates, and design confirmations, please contact the technical office.",RS04/11-BV +  2620M-BV-BAM,"Assembly
",>90,,Olev,3.000000000000,"BEAM STICK NUANCE BALLOTON Ø350
",1500.000000000000,1.000000000000,1500.000000000000,1.000000000000
W,9.290304000000,1,1,60.000000000000,1,1,0,Oleve_2627,200.000000000000,0,1,generic,2627W-OR-BO-VBI,,109.816910733408,1380.000000000000,1,0,,1,1,0,,3000.000000000000,,11.820593893742,350.000000000000,0,148.541963750594,0,16777215,1,3048.000000000000,https://www.olevlight.com/categorie-prodotti/,"sospensione
",W,220-240V,"1x13.8W, 1x6.1W, 220-240V, 3000K- Canopy Rich gold| Body Super-matt white| Glass Glass: white",1230.000000000000,"1x13.8W, 1x6.1W","1x1979lm, 1x711lm","The BIM object is a non-detailed graphical representation of the product. For further details, updates, and design confirmations, please contact the technical office.",RS04/11-OR +  2620W-BO-VBI,"Assembly
",>90,,Olev,4.000000000000,"BEAM STICK NUANCE BALLOTON Ø350
",1500.000000000000,3.000000000000,1500.000000000000,4.000000000000
