,Wattage##ELECTRICAL_WATTAGE##WATTS,Voltage Loss##OTHER##,Total Light Loss Factor##OTHER##,Tilt Angle##ANGLE##DECIMAL DEGREES,Temperature Loss##OTHER##,Temperature Color##OTHER##,Surface Depreciation Loss##OTHER##,Photometric Web File##OTHER##,None##OTHER##,Luminous Intensity##ELECTRICAL_LUMINOUS_INTENSITY##CANDELAS,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Luminaire Dirt Depreciation##OTHER##,Light Loss Input Method##OTHER##,Light Loss Factor##OTHER##,Lamp Tilt Loss##OTHER##,Lamp Lumen Depreciation##OTHER##,Initial Light Intensity Input Method##OTHER##,Initial Intensity##OTHER##,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Initial Color##OTHER##,Illuminance##ELECTRICAL_ILLUMINANCE##LUX,Emit from Line Length##LENGTH##MILLIMETERS,Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT,Dimming Lamp Color Temperature Shift##OTHER##,Color Filter##OTHER##,Temperature_W##OTHER##,Table##OTHER##,T##LENGTH##MILLIMETERS,Temperature_M##OTHER##,OLV_Code##OTHER##,Ballast Loss##OTHER##,URL##OTHER##,OLV_Type##OTHER##,OLV_Temperature##OTHER##,OLV_Supply##OTHER##,OLV_Supplementary_Description##OTHER##,OLV_Price##CURRENCY##CURRENCY,OLV_Power##OTHER##,OLV_Nominal lumen##OTHER##,OLV_Disclaimer##OTHER##,OLV_Composed_by##OTHER##,OLV_Code_Type##OTHER##,OLV_CRI##OTHER##,Model##OTHER##,Manufacturer##OTHER##,G##LENGTH##MILLIMETERS,Description##OTHER##,At a distance##LENGTH##MILLIMETERS,Actual Cable length##LENGTH##MILLIMETERS,C##LENGTH##MILLIMETERS,Cable length##LENGTH##MILLIMETERS,B##LENGTH##MILLIMETERS
W,9.290304000000,1,1,60.000000000000,1,0,1,generic,,109.816910733408,1380.000000000000,1,0,,1,1,0,,3000.000000000000,,11.820593893742,609.600000000000,148.541963750594,0,16777215,1,Oleve_2603,200.000000000000,0,2603W-RR-OR-VFU,1,https://www.olevlight.com/,"sospensione
",W,220-240V,"1x15.0W, 1x4.2W, 220-240V, 3000K- Canopy Pink copper| Body Rich gold| Glass Glass: smoke grey",856.000000000000,"1x15.0W, 1x4.2W","1x2760lm, 1x727lm","The BIM object is a non-detailed graphical representation of the product. For further details, updates, and design confirmations, please contact the technical office.",RS04/02-RR +  2612W-OR-VFU,"Assembly
",>90,,Olev,6.000000000000,CURUBA,3048.000000000000,800.000000000000,5.000000000000,800.000000000000,4.000000000000
M,9.290304000000,1,1,60.000000000000,1,0,1,generic,,109.816910733408,1380.000000000000,1,0,,1,1,0,,2700.000000000000,,11.820593893742,609.600000000000,148.541963750594,0,16777215,0,Oleve_2603,100.000000000000,1,2603M-BO-NO-BTM,1,https://www.olevlight.com/,"sospensione
",M,220-240V,"1x15.0W, 1x4.2W, 220-240V, 2700K- Canopy Super-matt white| Body Super-matt black| Glass Glass: Balloton brown",856.000000000000,"1x15.0W, 1x4.2W","1x2720lm, 1x727lm","The BIM object is a non-detailed graphical representation of the product. For further details, updates, and design confirmations, please contact the technical office.",RS04/02-BO +  2612M-NO-BTM,"Assembly
",>90,,Olev,1.000000000000,CURUBA,3048.000000000000,800.000000000000,1.000000000000,800.000000000000,2.000000000000
